SIMISA@@@@@@@@@@JINX0D0t______

Wagon (
	230BV2 
	Type ( Engine )
	WagonShape ( 230BV2.s )
	
	Size ( 2.809m 4.196m 11.0m )
	CentreOfGravity ( 0m 1.7m 0m )
	Centre ( 0m 0m 0m )
	Mass ( 82t )
	InertiaTensor (
		Box ( 2.809m 4.196m 11.0m )
	)
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 4e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			Break ( 5e7N 5e7N )
			r0 ( 10cm 10cm )
		)
		CouplingHasRigidConnection ( 1 )
		Velocity ( 0.1m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 5e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	Adheasion ( 0.3 0.5 2 0.5 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 240kN )
	DerailBufferForce ( 400kN )
	WheelRadius ( 1.045m )
	NumWheels ( 10 )
	Friction ( 50N/m/s 1 -1mph 0 1 5.1N/rad/s 1 -1rad/s 0 1 )
	BrakeEquipmentType ( "Triple_valve, Auxilary_reservoir, Handbrake" )
	BrakeSystemType ( "Air_single_pipe" )
	MaxBrakeForce ( 100kN )
	MaxHandbrakeForce ( 90kN )
	NumberOfHandbrakeLeverSteps ( 100 )
	TripleValveRatio ( 2.5 )
	MaxReleaseRate ( 15 )
	MaxApplicationRate ( 15 )
	MaxAuxilaryChargingRate ( 15 )
	BrakeCylinderPressureForMaxBrakeBrakeForce ( 70 )
	Lights (
		4 
		Light (
			comment ( Lueur Foyer )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 0 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States (
				2 
				State (
					Duration ( 0.05 )
					LightColour ( 80ff7200 )
					Position ( 0 2.2 -4.0 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 1.4 )
				)
				State (
					Duration ( 0.05 )
					LightColour ( 80ffe610 )
					Position ( 0 2.2 -4.0 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 1.4 )
				)
			)
		)
		Light (
			comment ( Sphere of light )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
			)
			Cycle ( 0 )
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States (
				1 
				State (
					Duration ( 0.0 )
					LightColour ( ffffffd5 )
					Position ( 0 10 0 )
					Transition ( 0 )
					Radius ( 160.0 )
					Angle ( 12 )
				)
			)
		)
		Light (
			comment ( Lanterne sur traverse )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States (
				1 
				State (
					Duration ( 0.0 )
					LightColour ( cdffffd5 )
					Position ( -1.05 1.61 5.15 )
					Azimuth ( 0.0 0.0 5.0 )
					Transition ( 0 )
					Radius ( 1.0 )
				)
			)
		)
		Light (
			comment ( Lanterne sur traverse )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States (
				1 
				State (
					Duration ( 0.0 )
					LightColour ( ffffffff )
					Position ( -1.05 1.61 5.15 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0 )
					Radius ( 1.0 )
				)
			)
		)
	)
	Sound ( "242A1Eng.sms" )
)
Engine (
	230BV2 
	Effects (
		SteamSpecialEffects (
			comment ( the format of these little blocks is as follow: offset.x offset.y offset.z normal.x normal.y normal.z width in metres defining the offset from the shape pivot point where steam / smoke should appear, the direction it should go and the width of the nozzle )
			WhistleFX ( 0 4.32 -3.65 0 1 0 0.12 )
			SafetyValvesFX ( 0 4.32 -3.65 0 1 0 0.12 )
			StackFX ( 0 4.4 3.1 0 1 0 0.16 )
			DrainpipeFX ( -1.5 1.26 -3.9 -0.4 -1 -0.2 0.05 )
			CylindersFX ( -1.2 0.35 1.7 0 0 1 0.05 )
			CylindersFX ( 1.2 0.35 1.7 0 0 1 0.05 )
		)
	)
	Wagon ( 230BV2 )
	Type ( Steam )
	MaxPower ( 880KW)
	MaxForce ( 140KN )
	MaxVelocity ( 105kmh )
	IsTenderRequired ( 1 )
	WheelRadius ( 0.71m )
	Sanding ( 1e20kmh )
	NumWheels ( 4 )
	BoilerLength ( 6.0m )
	BoilerVolume ( "160*(ft^3)" )
	BoilerEffectivity ( 1.26 )
	DraftingEffect ( 0.8 )
	BoilerResponsiveness ( 1.25 )
	CoalBurnage ( 1.75lb/hp/h )
	MaxBoilerOutput ( 34500lb/h )
	NumCylinders ( 2 )
	CylinderStroke ( 26in )
	CylinderDiameter ( 19in )
	CylinderVolume ( "22.12*(ft^3)" )
	CylinderEffectivity ( 1 )
	InjectorSizes ( 16mm 16mm )
	ExhaustLimit ( 35500lb/h )
	PrimingFactor ( 1 )
	SteamMinPrimingLevel ( 0.9 )
	BlastExponent ( 0.95 )
	MaxBoilerPressure ( 218psi )
	MaxFireMass ( 3500lb )
	IdealFireMass ( 2500lb )
	MaxWaterMass ( 4200lb )
	SafetyValvesSteamUsage ( 15000lb/h )
	ShovelCoalMass ( 11lb )
	SmokeCombustion ( 1 )
	MaxTenderCoalMass ( 8000lb )
	MaxTenderWaterMass ( 26000lb )
	comment ( 0 for live steam, 1 for exhaust steam )
	InjectorTypes ( 0 0 )
	Injector1FeedRateMultiplierExhaue ( 1.5 )
	Injector1FeedRateMultiplierLive ( 1.5 )
	Injector2FeedRateMultiplierExhaue ( 1.5 )
	Injector2FeedRateMultiplierLive ( 1.5 )
	Injector1WaterValveVariance ( 1 )
	Injector2WaterValveVariance ( 1 )
	SuperHeater ( 1.15 )
	SteamSmokeUnitsPerPoundOfFuel ( 8 )
	SteamMaxSmokeUnitsReleaseRate ( 10 )
	SteamFiremanMaxPossibleFiringRate ( 7000 )
	SteamGaugeGlassHeight ( 11 )
	MaxSteamHeatingPressure ( 80 )
	SafetyValvePressureDifference ( 5 )
	BasicSteamUsage ( 1400lb/h )
	BasicCoalUsage ( 1000lb/h )
	InjectorLimits1 ( 50psi 0.5 1 )
	InjectorLimits2 ( 50psi 0.5 1 )
	CylinderCocksPowerEfficiency ( 0.8 )
	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesProportionalBrakeLag ( 0.9 )
	TrainBrakesControllerMaxPressureDropInNormalApplication ( 70 )
	BrakesEngineBrakeType ( "Air_single_pipe" )
	BrakesTrainBrakeType ( "Air_single_pipe" )
	BrakesEngineControllers ( "Hand, Train, Independent" )
	SteamCylinderCocksOperation ( Manual )
	SteamSmallestCutoff ( 0.08 )
	NumberOfDamperSteps ( 4 )
	RegulatorValveType ( Twin_port )
	RegulatorSecondValveStartPosition ( 0.45 )
	RegulatorPilotValveExponent ( 1.7 )
	RegulatorSecondValveExponent ( 1.7 )
	RegulatorPilotValveFullOpenning ( 0.35 )
	RegulatorMainValveInitialOpenning ( 0.475 )
	SteamBlowerEffectExponent ( 0.9 )
	SteamBlowerEfficiencyExponent ( 1.1 )
	comment ( lbs/h )
	SteamBlowerMaxSteamUsageRate ( 500 )
	SteamBlowerMaxProportionOfBlastEffect ( 0.15 )
	AirBrakesAirCompressorPowerRating ( 3 )
	AirBrakesMainMinResAirPressure ( 0 )
	AirBrakesMainMaxAirPressure ( 100 )
	AirBrakesMainResVolume ( 8 )
	AirBrakesCompressorRestartPressure ( 95 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 0.25 )
	EngineBrakesControllerHasProportionalBrake ( 1 )
	TrainBrakesControllerMaxApplicationRate ( 5 )
	TrainBrakesControllerMaxReleaseRate ( 10 )
	TrainBrakesControllerEmergencyApplicationRate ( 10 )
	TrainBrakesControllerMinSystemPressure ( 0 )
	TrainBrakesControllerMaxSystemPressure ( 70 )
	EngineBrakesControllerMaxApplicationRate ( 6 )
	EngineBrakesControllerMaxReleaseRate ( 6 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 70 )
	CabView ( "130B_V2.cvf" )
	HeadOut ( -1.60 2.43 -4.4)
	EngineControllers (
		Regulator (
			0 1 0.025 0 
			NumNotches ( 0 )
		)
		Cutoff (
			-1.00 1.00 0.01 0 
			NumNotches ( 0 )
		)
		Brake_Engine (
			0 1 0.0125 0 
			NumNotches (
				3 
				Notch ( 0 1 EngineBrakesControllerReleaseStart )
				Notch ( 0.45 1 EngineBrakesControllerHoldStart )
				Notch ( 0.5 1 EngineBrakesControllerApplyStart )
			)
		)
		Brake_Train (
			0 1 0.0225 0.6 
			NumNotches (
				4 
				Notch ( 0 1 TrainBrakesControllerReleaseStart )
				Notch ( 0.4 0 TrainBrakesControllerSelfLapStart )
				Notch ( 0.5 1 TrainBrakesControllerApplyStart )
				Notch ( 0.9 1 TrainBrakesControllerEmergencyStart )
			)
		)
		Brake_Hand (
			0 1 0.0125 0 
			NumNotches ( 0 )
		)
		FireDoor (
			0 1 0.1 0 
			NumNotches ( 0 )
		)
		Sanding ( 0 1 0 )
		Blower (
			0 1 0.025 0.2 
			NumNotches ( 0 )
		)
		HeatingTap (
			0 1 0.1 0 
			NumNotches ( 0 )
		)
		Shovel (
			0 1 0.1 0 
			NumNotches ( 0 )
		)
		DampersFront (
			0 1 0.1 1 
			NumNotches ( 0 )
		)
		DampersBack (
			0 1 0.1 0 
			NumNotches ( 0 )
		)
		Injector1Steam ( 0 1 0 )
		Injector2Steam ( 0 1 0 )
		Injector1Water (
			0 1 0.1 0 
			NumNotches ( 0 )
		)
		Injector2Water (
			0 1 0.1 0 
			NumNotches ( 0 )
		)
		CylinderCocks ( 0 1 1 )
		Whistle ( 0 1 0 )
		SmallEjectorOrCompressor ( 0 1 1 )
		BellToggle ( 0 1 0 )
		Headlights ( 0 1 0 )
	)
	comment ( fire temp, fire mass, water mass, boiler pressure, tender_water_mass, tender_coal_mass, smoke_quantity, fire_condition, coal quality )
	EngineVariables ( 700 1450 4200 130 48395 15400 350 1 1 )
	Sound ( "242A1cab.sms" )
	Name ( "230BV2" )
	Description ( "Locomotive à vapeur du type 230 Atlantic Année de construction 1921 Schneider et Sté Alsacienne pour le réseau de l'Etat\n\n\n\n"+
		"Configuration des roues : Huit roues motrices de 165 cm de diamètre, configuration 141\n\n"+
		"Pression maxi de la chaudière : 14 kg/cm² (199.08 psi)\n\n"+
		"Vitesse maxi (autorisée) : 62 mph (100 km/h)/h\n\n"+
		"Hauteur : 4,27 m\n\n"+
		"Largeur : 2,98 m\n\n"+
		"Longueur : locomotive : 13.755m\n\n"+
		"Poids :89.200 tonnes\n\n"+
		"Puissance 1800ch\n\n"+
		"Effort de traction : 22.83tonnes\n\n"+
		"Capacité en charbon : 7 tonnes\n\n"+
		"Capacité en eau : 22000 litres\n\n"+
		"Freins : à air\n\n" )
	EngineOperatingProcedures ( "Pour avancer\n"+
		"1.	Appuyez plusieurs fois sur la touche W pour déplacer le levier d'inversion entièrement vers l'avant.\n"+
		"2.	Appuyez sur la touche M pour désactiver les freins de train.\n"+
		"3.	Appuyez sur la touche ^ (ACCENT CIRCONFLEXE) pour désactiver le frein de locomotive.\n"+
		"4.	Appuyez sur la touche D pour augmenter la valeur d'inversion.\n"+
		"5.	Pendant que vous accélérez, appuyez sur la touche S pour diminuer lentement la valeur d'inversion, puis réglez le régulateur pour conserver la vitesse souhaitée.\n\n"+
		"Pour ralentir le train\n"+
		"1.	Appuyez sur la touche Q pour placer le régulateur sur une position plus basse.\n"+
		"2.	Utilisez les freins pour réduire encore la vitesse si vous le souhaitez.\n\n"+
		"Pour activer les freins de train\n"+
		"1.	Appuyez sur la touche ' (APOSTROPHE) pour activer les freins de train.\n\n"+
		"Pour désactiver les freins de train\n"+
		"1. Appuyez sur la touche M pour désactiver les freins de train.\n\n"+
		"Pour activer le frein de locomotive\n"+
		"1.	Appuyez sur la touche $ pour activer le frein de locomotive.\n\n"+
		"Pour désactiver le frein de locomotive\n"+
		"1. Appuyez sur la touche ^ (ACCENT CIRCONFLEXE) pour désactiver le frein de locomotive.\n\n"+
		"Pour faire marche arrière\n"+
		"1.	Immobilisez complètement le train.\n"+
		"2.	Appuyez plusieurs fois sur la touche S pour déplacer le levier d'inversion entièrement vers la marche arrière.\n"+
		"3.	Appuyez sur la touche M pour désactiver les freins.\n"+
		"4.	Avancez lentement le régulateur (touche D).\n\n"+
		"Pour embarquer/débarquer des passagers\n"+
		"1. Arrêtez-vous dans une gare.\n"+
		"2. Appuyez sur la touche ENTRÉE.\n"+
		"3. Attendez le \"permission to depart\" coup de sifflet.\n"+
		"CONSEIL : Utilisez l'outil d'aide à la conduite de la prochaine gare (F10) pour contrôler l'embarquement et le débarquement.\n\n"+
		"Pour atteler un wagon ou une locomotive\n"+
		"1. Allez en roue libre vers l'unité à très basse vitesse, environ 6 km/h.\n"+
		"CONSEIL : Pour utiliser la vue de l'attelage, appuyez sur la touche - (TIRET).\n"+
		"2. Appuyez sur F9 pour ouvrir la fenêtre Opérations ferroviaires.\n"+
		"3. Si l'icône de l'unité à dételer est rouge, le frein à main est activé. Double-cliquez sur la voiture pour désactiver le frein à main.\n"+
		"4. Fermez la fenêtre Opérations ferroviaires.\n\n"+
		"Pour dételer un wagon ou une locomotive\n"+
		"1. Appuyez sur F9 pour ouvrir la fenêtre Opérations ferroviaires.\n"+
		"2. Double-cliquez sur une unité de la partie du train à dételer de la locomotive pour activer le frein à main.\n"+
		"3. Double-cliquez sur l'attelage qui se trouve entre les unités à dételer et le reste du train.\n"+
		"4. Cliquez sur « l'attelage » vert entre les deux unités à dételer.\n"+
		"5. Cliquez sur le bouton Dételer.\n"+
		"6. Fermez la fenêtre Opérations ferroviaires.\n\n"+
		"Commandes de chauffage (Chauffeur automatique désactivé dans l'écran Options)\n"+
		"Pour ajouter du charbon dans le foyer\n"+
		"1. Appuyez sur la touche F pour ouvrir la porte du foyer.\n"+
		"2. Appuyez sur la touche R pour augmenter la cadence du pelletage.\n\n"+
		"Pour cesser d'ajouter du charbon dans le feu\n"+
		"1. Appuyez sur MAJ+R pour diminuer la cadence du pelletage.\n"+
		"2. Appuyez sur MAJ+F pour fermer la porte du foyer.\n"+
		"Pour utiliser le souffleur\n\n"+
		"1.	Appuyez sur la touche N pour augmenter l'intensité du souffleur.\n"+
		"2. Appuyez sur MAJ+N pour diminuer l'intensité du souffleur.\n\n"+
		"Pour utiliser les registres\n"+
		"1.	Appuyez sur la touche , (VIRGULE) pour ouvrir les registres.\n"+
		"2. Appuyez sur MAJ+M pour fermer les registres.\n\n"+
		"Pour injecter de l'eau dans la chaudière\n"+
		"1.	Appuyez sur la touche I pour activer la vapeur de l'injecteur 1.\n"+
		"(Vous pouvez aussi appuyer sur la touche O pour activer la vapeur de l'injecteur 2.)\n"+
		"2.	Appuyez sur la touche K pour augmenter le débit d'eau de l'injecteur 1.\n"+
		"(Pour augmenter le débit d'eau de l'injecteur 2, appuyez sur la touche L.)\n\n"+
		"Pour cesser d'injecter de l'eau dans la chaudière\n"+
		"1. Appuyez sur la touche K pour désactiver la vapeur de l'injecteur 1.\n"+
		"2. Appuyez sur la touche O pour désactiver la vapeur de l'injecteur 2." )
	OverspeedMonitor (
		MonitoringDeviceTriggerOnTrackOverspeed ( 0 )
	)
)
