SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( Tender22A
	Type ( Tender )
	WagonShape ( Tender22A.s )
	Size ( 2.615m 4.235m 7.3m )
	CentreOfGravity ( 0m 1.6 m 0m )
	Mass ( 32.4t)
	InertiaTensor ( Box ( 2.615m 4.235m 7.3m ) )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 1e6N/m 2e6N/m )
			Damping ( 1e7N/m 1e7N/m)
			Break ( 3.2e6N 3.2e6N )
			r0 ( 10cm 10cm )
		)
	)
	Lights	(	2
				
		Light	(
			comment( Lanterne rouge droite )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 3 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 1.10 1.76 -2.8 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 1.0 )
				)
			)
		)
		Light	(
			comment( Lanterne rouge )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 3 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -1.10 1.76 -2.8 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 1.0 )
				)
			)
		)

	)
	BrakeEquipmentType( "Handbrake, Vacuum_brake, Auxilary_reservoir" )
	BrakeSystemType( "Vacuum_single_pipe" )
	MaxBrakeForce( 54kN )

	MaxHandbrakeForce( 27kN )
	AuxilaryLeakRate( 0.1 )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 14 )
	MaxApplicationRate( 14 )
	MaxAuxilaryChargingRate( 15 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 20 )
	
	Adheasion ( 0.2 0.4 2 0 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 150kN)
	DerailBufferForce ( 400kN )
	WheelRadius ( 0.45m )
	NumWheels (	2 )
	Friction (
		325N/m/s			0		1mph		2.85N/m/s		1.8
		5.1N/rad/s		1		-1rad/s		0		1
	)
	IntakePoint (1.60 1.0 FuelWater )
	IntakePoint ( -0.80 1.80 FuelCoal )
    	
    	Sound ( "genfreightwag1.sms" )
)

