SIMISA@@@@@@@@@@JINX0D0t______

Wagon (
	230TAEst
	Type ( Engine )
	WagonShape ( 230TAEst-anim.s )
	FreightAnim ( 230TARst_FA.s 1 1 )
      Size ( 3.005m 4.195m 12.052m )
	Mass ( 64.5t )
	InertiaTensor (Box ( 3.005m 4.195m 12.052m ))
	
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 5e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			Break ( 2e7N 2e7N )
			r0 ( 20cm 30cm )
		)
		CouplingHasRigidConnection ( 1 )
		Velocity ( -0.1m/s )
	)
	Adheasion ( 0.15 0.3 2 0.5 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 240kN )
	DerailBufferForce ( 400kN )
	WheelRadius ( 0.875m )
	NumWheels ( 10 )
	Friction ( 50N/m/s 1 -1mph 0 1 5.1N/rad/s 1 -1rad/s 0 1 )
	BrakeEquipmentType ( "Triple_valve, Auxilary_reservoir, Handbrake" )
	BrakeSystemType ( "Air_single_pipe" )
	MaxBrakeForce ( 100kN )
	MaxHandbrakeForce ( 90kN )
	NumberOfHandbrakeLeverSteps ( 100 )
	TripleValveRatio ( 2.5 )
	MaxReleaseRate ( 15 )
	MaxApplicationRate ( 15 )
	MaxAuxilaryChargingRate ( 15 )
	BrakeCylinderPressureForMaxBrakeBrakeForce ( 70 )
	
	Lights ( 8

 
		Light (
			comment ( Sphere of light )
			Type ( 1 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
			)
			Cycle ( 0 )
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States (
				1 
				State (
					Duration ( 0.0 )
					LightColour ( ffffffd5 )
					Position ( 0.0 10 0 )
					Transition ( 0 )
					Radius ( 300.0 )
					Angle ( 60.0 )
				)
			)
		)
		Light (
			comment ( Sphere of light )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
			)
			Cycle ( 0 )
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States (
				1 
				State (
					Duration ( 0.0 )
					LightColour ( ffffffd5 )
					Position ( 0.0 10 0 )
					Transition ( 0 )
					Radius ( 500.0 )
					Angle ( 90.0 )
				)
			)
		)
		Light (
			comment ( Head light right dim )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States (
				1 
				State (
					Duration ( 0.0 )
					LightColour ( cdffffd5 )
					Position ( -1.0 1.64 5.75 )
					Azimuth ( 0.0 0.0 5.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( Head light right dim )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States (
				1 
				State (
					Duration ( 0.0 )
					LightColour ( cdffffd5 )
					Position ( -1.0 1.64 5.75 )
					Azimuth ( 0.0 0.0 5.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( Head light left dim )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States (
				1 
				State (
					Duration ( 0.0 )
					LightColour ( cdffffd5 )
					Position ( 1.0 1.64 5.75 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( Head light left dim )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States (
				1 
				State (
					Duration ( 0.0 )
					LightColour ( cdffffd5 )
					Position ( 1.0 1.64 5.75 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( Head light left red )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 3 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States (
				1 
				State (
					Duration ( 0.0 )
					LightColour ( cdff0000 )
					Position ( -0.96 1.95 -5.7 )
					Azimuth ( 180.0 180.0 180.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Head light left red )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 3 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States (
				1 
				State (
					Duration ( 0.0 )
					LightColour ( cdff0000 )
					Position ( -0.96 1.95 -5.7 )
					Azimuth ( 180.0 180.0 180.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
	)
	Sound ( "242A1eng.sms" )
)
Engine (
	230TAEst 
	Effects (
		SteamSpecialEffects (
			comment ( the format of these little blocks is as follow: offset.x offset.y offset.z normal.x normal.y normal.z width in metres defining the offset from the shape pivot point where steam / smoke should appear, the direction it should go and the width of the nozzle )
			WhistleFX ( 0 4 -3.3 0 1 0 0.05 )
			SafetyValvesFX ( 0 4 -0.5 0 1 0 0.2 )
			StackFX ( 0 4.3 3.8 0 1 0 0.2 )
			DrainpipeFX ( -1.5 1.258 -1.82 -0.4 -1 -0.2 0.05 )
			CylindersFX ( -1.223 0.71 3.5 0 0 1 0.05 )
			CylindersFX ( 1.223 0.71 3.5 0 0 1 0.05 )
		)
	)
	Wagon ( 230TAEst )
	Type ( Steam )
	MaxPower ( 420kW )
	MaxForce ( 110kN )
	MaxVelocity ( 90km/h )
	comment (IsTenderRequired ( 1 ))
	WheelRadius ( 0.71m )
	Sanding ( 1e9mph )
	NumWheels ( 2 )
	BoilerLength ( 7.0m )
	BoilerVolume ( "170*(ft^3)" )
	BoilerEffectivity ( 1.26 )
	DraftingEffect ( 0.8 )
	BoilerResponsiveness ( 1.23 )
	CoalBurnage ( 1.75lb/hp/h )
	MaxBoilerOutput ( 34500lb/h )
	NumCylinders ( 2 )
	CylinderStroke ( 26in )
	CylinderDiameter ( 19in )
	CylinderVolume ( "22.12*(ft^3)" )
	CylinderEffectivity ( 1 )
	InjectorSizes ( 12mm 12mm )
	ExhaustLimit ( 35500lb/h )
	PrimingFactor ( 1 )
	BlastExponent ( 0.95 )
	MaxBoilerPressure ( 218psi )
	MaxFireMass ( 3500lb )
	IdealFireMass ( 2500lb )
	MaxWaterMass ( 4200lb )
	SafetyValvesSteamUsage ( 15000lb/h )
	ShovelCoalMass ( 1lb )
	SmokeCombustion ( 1 )
	SteamSmokeUnitsPerPoundOfFuel ( 5.5 )
	MaxTenderCoalMass ( 18000lb )
	MaxTenderWaterMass ( 50000lb )
	comment ( 0 for live steam, 1 for exhaust steam )
	InjectorTypes ( 0 0 )
	SuperHeater ( 1.15 )
	SteamFiremanMaxPossibleFiringRate ( 7000 )
	SteamGaugeGlassHeight ( 11 )
	MaxSteamHeatingPressure ( 80 )
	SafetyValvePressureDifference ( 5 )
	BasicSteamUsage ( 1400lb/h )
	BasicCoalUsage ( 1000lb/h )
	InjectorLimits1 ( 50psi 0.5 1 )
	InjectorLimits2 ( 50psi 0.5 1 )
	CylinderCocksPowerEfficiency ( 0.8 )
	TrainBrakesControllerMaxReleaseRate ( 10 )
	TrainBrakesControllerMaxApplicationRate ( 10 )
	TrainBrakesControllerEmergencyApplicationRate ( 35 )
	TrainBrakesControllerMinSystemPressure ( 0 )
	TrainBrakesControllerMaxSystemPressure ( 70 )
	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesProportionalBrakeLag ( 0.9 )
	TrainBrakesControllerMaxPressureDropInNormalApplication ( 70 )
	BrakesEngineBrakeType ( "Air_single_pipe" )
	BrakesTrainBrakeType ( "Air_single_pipe" )
	BrakesEngineControllers ( "Hand, Train, Independent" )
	SteamCylinderCocksOperation ( Manual )
	SteamSmallestCutoff ( 0.08 )
	NumberOfDamperSteps ( 4 )
	RegulatorValveType ( Twin_port )
	RegulatorSecondValveStartPosition ( 0.45 )
	RegulatorPilotValveExponent ( 1.7 )
	RegulatorSecondValveExponent ( 1.7 )
	RegulatorPilotValveFullOpenning ( 0.35 )
	RegulatorMainValveInitialOpenning ( 0.475 )
	SteamBlowerEffectExponent ( 0.9 )
	SteamBlowerEfficiencyExponent ( 1.1 )
	comment ( lbs/h )
	SteamBlowerMaxSteamUsageRate ( 500 )
	SteamBlowerMaxProportionOfBlastEffect ( 0.15 )
	AirBrakesAirCompressorPowerRating ( 3 )
	AirBrakesMainMinResAirPressure ( 0 )
	AirBrakesMainMaxAirPressure ( 100 )
	AirBrakesMainResVolume ( 8 )
	AirBrakesCompressorRestartPressure ( 95 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 0.25 )
	EngineBrakesControllerHasProportionalBrake ( 1 )
	TrainBrakesControllerMaxApplicationRate ( 5 )
	TrainBrakesControllerMaxReleaseRate ( 10 )
	TrainBrakesControllerEmergencyApplicationRate ( 10 )
	TrainBrakesControllerMinSystemPressure ( 0 )
	TrainBrakesControllerMaxSystemPressure ( 70 )
	EngineBrakesControllerMaxApplicationRate ( 6 )
	EngineBrakesControllerMaxReleaseRate ( 6 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 70 )
	
	CabView ( "230TA.cvf" )
	HeadOut ( -2 3.2 -5.5 )
	EngineControllers (
		Regulator (
			0 1 0.025 0 
			NumNotches ( 0 )
		)
		Cutoff (
			-0.89 0.89 0.01 0 
			NumNotches ( 0 )
		)
		Brake_Engine (
			0 1 0.0125 0 
			NumNotches (
				3 
				Notch ( 0 1 EngineBrakesControllerReleaseStart )
				Notch ( 0.45 1 EngineBrakesControllerHoldStart )
				Notch ( 0.5 1 EngineBrakesControllerApplyStart )
			)
		)
		Brake_Train (
			0 1 0.0125 0.6 
			NumNotches (
				4 
				Notch ( 0 1 TrainBrakesControllerReleaseStart )
				Notch ( 0.4 1 TrainBrakesControllerSelfLapStart )
				Notch ( 0.5 1 TrainBrakesControllerApplyStart )
				Notch ( 0.9 1 TrainBrakesControllerEmergencyStart )
			)
		)
		Brake_Hand (
			0 1 0.0125 0 
			NumNotches ( 0 )
		)
		FireDoor (
			0 1 0.1 0 
			NumNotches ( 0 )
		)
		Sanding ( 0 1 0 )
		Blower (
			0 1 0.025 0.2 
			NumNotches ( 0 )
		)
		HeatingTap (
			0 1 0.1 0 
			NumNotches ( 0 )
		)
		Shovel (
			0 1 0.1 0 
			NumNotches ( 0 )
		)
		DampersFront (
			0 1 0.1 1 
			NumNotches ( 0 )
		)
		DampersBack (
			0 1 0.1 0 
			NumNotches ( 0 )
		)
		Injector1Steam ( 0 1 0 )
		Injector2Steam ( 0 1 0 )
		Injector1Water (
			0 1 0.1 0 
			NumNotches ( 0 )
		)
		Injector2Water (
			0 1 0.1 0 
			NumNotches ( 0 )
		)
		CylinderCocks ( 0 1 1 )
		Whistle ( 0 1 0 )
		SmallEjectorOrCompressor ( 0 1 1 )
		BellToggle ( 0 1 0 )
		Headlights ( 0 1 0 )
	)
	comment ( fire temp, fire mass, water mass, boiler pressure, tender_water_mass, tender_coal_mass, 	smoke_quantity, fire_condition, coal quality )
	EngineVariables ( 770 2650 3750 200 50000 18000 350 1 1 )
	Sound ( "242A1cab.sms" )
	Name ( "230TAEst" )
	Description ( "La locomotive à vapeur 230-TA_Est, conçue par le célèbre créateur de locomotives autrichien Karl Gölsdorf. L'effort de traction utile élevé de la 380 en fait l'outil idéal pour tirer le train de passagers .\n\n"+
		"Type de locomotive : Series 230TAEst (2-3-0)\n\n"+
		"Configuration des roues : dix roues motrices de 141 cm de diamètre, configuration 1E\n\n"+
		"Pression maxi de la chaudière : 16 kg/cm² (228 psi)\n\n"+
		"Vitesse maxi (autorisée) : 43.5 mph (90 km/h)/h\n\n"+
		"Hauteur : 4,57 m\n\n"+
		"Largeur : 3,08 m\n\n"+
		"Longueur : locomotive : 12,052m\n\n"+
		"Poids (locomotive) : 142 tonnes\n\n"+
		"Poids maxi sur les roues motrices : 14 tonnes\n\n"+
		"Effort de traction : 12,1 tonnes\n\n"+
		"Capacité en charbon : 10,2 tonnes\n\n"+
		"Capacité en eau : 29 500 litres\n\n"+
		"Freins : à air\n\n" )
	EngineOperatingProcedures ( "Pour avancer\n"+
		"1.	Appuyez plusieurs fois sur la touche W pour déplacer le levier d'inversion entièrement vers l'avant.\n"+
		"2.	Appuyez sur la touche M pour désactiver les freins de train.\n"+
		"3.	Appuyez sur la touche ^ (ACCENT CIRCONFLEXE) pour désactiver le frein de locomotive.\n"+
		"4.	Appuyez sur la touche D pour augmenter la valeur d'inversion.\n"+
		"5.	Pendant que vous accélérez, appuyez sur la touche S pour diminuer lentement la valeur d'inversion, puis réglez le régulateur pour conserver la vitesse souhaitée.\n\n"+
		"Pour ralentir le train\n"+
		"1.	Appuyez sur la touche Q pour placer le régulateur sur une position plus basse.\n"+
		"2.	Utilisez les freins pour réduire encore la vitesse si vous le souhaitez.\n\n"+
		"Pour activer les freins de train\n"+
		"1.	Appuyez sur la touche ' (APOSTROPHE) pour activer les freins de train.\n\n"+
		"Pour désactiver les freins de train\n"+
		"1. Appuyez sur la touche M pour désactiver les freins de train.\n\n"+
		"Pour activer le frein de locomotive\n"+
		"1.	Appuyez sur la touche $ pour activer le frein de locomotive.\n\n"+
		"Pour désactiver le frein de locomotive\n"+
		"1. Appuyez sur la touche ^ (ACCENT CIRCONFLEXE) pour désactiver le frein de locomotive.\n\n"+
		"Pour faire marche arrière\n"+
		"1.	Immobilisez complètement le train.\n"+
		"2.	Appuyez plusieurs fois sur la touche S pour déplacer le levier d'inversion entièrement vers la marche arrière.\n"+
		"3.	Appuyez sur la touche M pour désactiver les freins.\n"+
		"4.	Avancez lentement le régulateur (touche D).\n\n"+
		"Pour embarquer/débarquer des passagers\n"+
		"1. Arrêtez-vous dans une gare.\n"+
		"2. Appuyez sur la touche ENTRÉE.\n"+
		"3. Attendez le \"permission to depart\" coup de sifflet.\n"+
		"CONSEIL : Utilisez l'outil d'aide à la conduite de la prochaine gare (F10) pour contrôler l'embarquement et le débarquement.\n\n"+
		"Pour atteler un wagon ou une locomotive\n"+
		"1. Allez en roue libre vers l'unité à très basse vitesse, environ 6 km/h.\n"+
		"CONSEIL : Pour utiliser la vue de l'attelage, appuyez sur la touche - (TIRET).\n"+
		"2. Appuyez sur F9 pour ouvrir la fenêtre Opérations ferroviaires.\n"+
		"3. Si l'icône de l'unité à dételer est rouge, le frein à main est activé. Double-cliquez sur la voiture pour désactiver le frein à main.\n"+
		"4. Fermez la fenêtre Opérations ferroviaires.\n\n"+
		"Pour dételer un wagon ou une locomotive\n"+
		"1. Appuyez sur F9 pour ouvrir la fenêtre Opérations ferroviaires.\n"+
		"2. Double-cliquez sur une unité de la partie du train à dételer de la locomotive pour activer le frein à main.\n"+
		"3. Double-cliquez sur l'attelage qui se trouve entre les unités à dételer et le reste du train.\n"+
		"4. Cliquez sur « l'attelage » vert entre les deux unités à dételer.\n"+
		"5. Cliquez sur le bouton Dételer.\n"+
		"6. Fermez la fenêtre Opérations ferroviaires.\n\n"+
		"Commandes de chauffage (Chauffeur automatique désactivé dans l'écran Options)\n"+
		"Pour ajouter du charbon dans le foyer\n"+
		"1. Appuyez sur la touche F pour ouvrir la porte du foyer.\n"+
		"2. Appuyez sur la touche R pour augmenter la cadence du pelletage.\n\n"+
		"Pour cesser d'ajouter du charbon dans le feu\n"+
		"1. Appuyez sur MAJ+R pour diminuer la cadence du pelletage.\n"+
		"2. Appuyez sur MAJ+F pour fermer la porte du foyer.\n"+
		"Pour utiliser le souffleur\n\n"+
		"1.	Appuyez sur la touche N pour augmenter l'intensité du souffleur.\n"+
		"2. Appuyez sur MAJ+N pour diminuer l'intensité du souffleur.\n\n"+
		"Pour utiliser les registres\n"+
		"1.	Appuyez sur la touche , (VIRGULE) pour ouvrir les registres.\n"+
		"2. Appuyez sur MAJ+M pour fermer les registres.\n\n"+
		"Pour injecter de l'eau dans la chaudière\n"+
		"1.	Appuyez sur la touche I pour activer la vapeur de l'injecteur 1.\n"+
		"(Vous pouvez aussi appuyer sur la touche O pour activer la vapeur de l'injecteur 2.)\n"+
		"2.	Appuyez sur la touche K pour augmenter le débit d'eau de l'injecteur 1.\n"+
		"(Pour augmenter le débit d'eau de l'injecteur 2, appuyez sur la touche L.)\n\n"+
		"Pour cesser d'injecter de l'eau dans la chaudière\n"+
		"1. Appuyez sur la touche K pour désactiver la vapeur de l'injecteur 1.\n"+
		"2. Appuyez sur la touche O pour désactiver la vapeur de l'injecteur 2." )
	OverspeedMonitor (
		MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
	)
)
