SIMISA@@@@@@@@@@JINX0D0t______

Wagon (  MB_231B
 Type ( Engine)
 Wagonshape ( MB_231B.s )
 FreightAnim ( MB_FA_231B.s 1 1 )
 Size ( 2.93m 4.295 m 14.373m)
 Centreofgravity ( 0m 2.15m 0m)
 Centre ( 0m 0m 0m)
 Mass ( 102t)
 InertiaTensor (
  Box ( 2.93m 4.295m 15.373m )
  )
 Coupling (
  Type ( Chain)
  Spring (
   Stiffness ( 4.5e6N/m 4.9e6N/m)
   Damping ( 1.2e6N/m/s 1.2e6N/m/s)
   Break ( 5.4e7N 5.4e7N)
   R0 ( 580cm 10cm)
  )
CouplingHasRigidConnection ( 1)
  Velocity ( 0.1m/s)
  )
  Buffers (
		Spring (
			Stiffness ( 5e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)

 Adheasion ( 0.2591   0.8205   0.9263   0 )
 DerailRailHeight ( 10cm)
 DerailRailForce ( 240kN)
 DerailBufferForce ( 400kN)
 Wheelradius ( 0.4825m)
 NumWheels(4)
 Friction (10670N/m/s   -0.10  6.0mph   10N/m/s 1.9
           5.1N/rad/s    1    -1rad/s   0       1 )

comment( Friction modified with TS-FastFix 1.0
   All equations from FCalc 2.0 by Joseph T. Realmuto.

   Rail Unit Type : Steam Locomotive
   Speed Range    : 95mph / 153kph
   Number of Axles: 3
   Weight         : 102.0t / 76.5t on powered axles = 75.0%
   Frontal Area   : 11.48m²
   Cd             : 1)
 BrakeEquipmentType ( "Triple_valve, Auxilary_reservoir, Handbrake")
 BrakeSystemType ( Air_single_pipe)
 MaxBrakeForce ( 71.4kN)
 MaxHandbrakeForce ( 80kN)
 NumberOfHandbrakeLeverSteps ( 100)
 TripleValveRatio( 2.5 )
 MaxReleaseRate( 20 )
 MaxApplicationRate( 20 )
 MaxAuxilaryChargingRate( 30 )
      BrakeCylinderPressureForMaxBrakeBrakeForce( 70 ) 
 Lights ( 4
  Light (
   Type ( 1 #Front sphere of Light)
   Conditions (
    Headlight ( 3)
    Unit ( 2)
   )
   Cycle ( 0)
   FadeIn ( 1)
   FadeOut ( 1)
   States ( 1
    State (
     Duration ( 0.0)
     LightColour ( ddffffcc)
     Position ( 0 3.4 7.0 )
     Transition ( 0)
     Radius ( 150.0)
     Angle ( 9.0)
    )
   )
  )

  Light (
   Comment( foyer )
   Type  ( 0 )
   Conditions (
    Headlight ( 0 )
    Unit ( 0 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 2
    State (
     Duration ( 0.07 )
     LightColour ( 80ff7200 )
     Position ( -0.1 2.45 -5.25 )
     Azimuth ( -180 -180 -180 )
                              Elevation ( -20 0 90 )
     Transition ( 0 )
     Radius ( 0.6 )
     )
    State (
     Duration ( 0.07 )
     LightColour ( 80ffe610 )
     Position ( -0 2.50 -5.25 )
     Azimuth ( -180 -180 -180 )
     Transition ( 0 )
                              Elevation ( -20 0 90 )
     Radius ( 0.6 )
         
    )
   )
  )

	Light (
	Comment ( Lanterne sur boite à fumée )
	Type ( 0 )
	Conditions (
		Headlight ( 3 )
		Unit ( 2 )
	)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1 
				State (
					Duration ( 0.0 )
					LightColour ( aaffffcc )
					Position ( 0 3.26 5.35 )
					Azimuth ( 0.0 0.0 5.0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
Light (
	Comment ( Lanterne sur boite à fumée )
	Type ( 0 )
	Conditions (
		Headlight ( 3 )
		Unit ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1 
				State (
					Duration ( 0.0 )
					LightColour ( aaffffcc )
					Position ( 0 3.06 5.35 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
     )

 
 Sound ( "231Geng.sms" )
)
Engine ( MB_231B
 Effects (
  SteamSpecialEffects (
   StackFX ( 0 4.6 4.2 0 1 0 0.22)
   CylindersFX ( -1.35 0.5 3.59 0 0 -1 0.1)
   CylindersFX ( 1.35 0.5 3.59 0 0 -1 0.1)
   WhistleFX ( 0 4.45 -4.94 0 1 0 0.1)
   SafetyValvesFX ( 0.0 4.5 -4.34 0 1 0 0.1)
   DrainpipeFX ( -1.5 1.258 -3.886 -0.4 -1 -0.2 0.05)
  )
 )
 Wagon ( MB_231B)
 Istenderrequired ( 1 )
 Type ( Steam )
 MaxPower ( 1860kW )
 MaxForce ( 140kN )
 MaxVelocity ( 81mph)
 Wheelradius (1.11m )
 Sanding ( 19mph )
 NumWheels(3)
 BoilerLength ( 6.5m )
 BoilerVolume ( "250*(ft^3)")
 BoilerEffectivity ( 0.9)
 DraftingEffect ( 0.9)
 BoilerResponsiveness ( 1.2)
 CoalBurnage ( 3.90b/hp/h)
 MaxBoilerOutput ( 32000lb/h)
 NumCylinders ( 4 )
 CylinderStroke ( 650mm)comment (BP)
 CylinderDiameter ( 640mm )comment (BP)
 CylinderStroke ( 650mm)comment (HP)
 CylinderDiameter ( 420mm )comment (HP)
 CylinderVolume ( "21.3* (ft^3)")
 Comment ( Machine compound,1/2 volume cyl.BP+HP)
 CylinderEffectivity ( 1.0 ) 
 ExhaustLimit ( 32000lb/h )
 PrimingFactor ( 1 )
 BlastExponent ( 0.85 )
 MaxBoilerPressure ( 232psi )
 MaxFireMass ( 2650lb )
 IdealFireMass ( 1900lb )
 MaxWaterMass ( 18700lb )
 SafetyValvesSteamUsage ( 8000lb/h)
 ShovelCoalMass ( 10lb )
 SteamFiremanMaxPossibleFiringRate ( 8000)
 SmokeCombustion ( 1)
 MaxTenderCoalMass ( 26450lb )
 MaxTenderWaterMass ( 48500lb )
 Comment ( 0 for live steam, 1 for exhaust steam )

 SuperHeater ( 1.23 )
 SteamSmokeUnitsPerPoundOfFuel ( 7 )
 SteamMaxSmokeUnitsReleaseRate ( 10 )
 MaxSteamHeatingPressure ( 80)
 SafetyValvePressureDifference ( 5)
 SteamGaugeGlassHeight ( 11)

 BasicSteamUsage ( 100lb/h)
 BasicCoalUsage ( 85lb/h)
 Comment ( min steam pressure, min water proportion, max water proportion)
 InjectorTypes ( 0 1)
 InjectorSizes ( 12mm 14mm)
 InjectorLimits1 ( 32psi 0.5 1)
 InjectorLimits2 ( 32.5psi 0.3 1)
 Injector1FeedRateMultiplierExhaust ( 0.1)
 Injector1FeedRateMultiplierLive ( 0.175)
 Comment ( steam usage)
 Injector2FeedRateMultiplierExhaust ( 0.5)
 Injector2FeedRateMultiplierLive ( 0.2)
 Comment ( steam usage)
 Injector1WaterValveVariance ( 0.75)
 Injector2WaterValveVariance ( 0.5)
 CylinderCocksPowerEfficiency ( 0.9)
 SteamCylinderCocksOperation ( Manual)

 BrakesEngineBrakeType ( Air_single_pipe)
 BrakesTrainBrakeType ( Air_single_pipe)
 BrakesEngineControllers ( "Hand, Train, Independent")
 AirBrakesAirCompressorPowerRating ( 3)
 AirBrakesMainMinResAirPressure ( 0)
 AirBrakesMainMaxAirPressure ( 100)
 AirBrakesMainResVolume ( 8)
 AirBrakesCompressorRestartPressure ( 95)
 AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 0.25)
 
 TrainBrakesControllerMaxPressureDropInNormalApplication ( 70)
 TrainBrakesControllerMaxReleaseRate ( 2)
 TrainBrakesControllerMaxApplicationRate ( 3)
 TrainBrakesControllerMinSystemPressure ( 0)
 TrainBrakesControllerMaxSystemPressure ( 100)
 
 EngineBrakesControllerHasProportionalBrake ( 1)
 EngineBrakesProportionalBrakeLag ( 1)
 EngineBrakesControllerMaxApplicationRate ( 6)
 EngineBrakesControllerMaxReleaseRate ( 6)
 EngineBrakesControllerMinSystemPressure ( 0)
 EngineBrakesControllerMaxSystemPressure ( 70)
 SteamSmallestCutoff ( 0.05)
 NumberOfDamperSteps ( 4)

 RegulatorValveType ( Twin_port)
 RegulatorSecondValveStartPosition ( 0.45)
 RegulatorPilotValveExponent ( 0.75)
 RegulatorPilotValveInitialOpening ( 0.08)
 RegulatorSecondValveExponent ( 1.25)
 RegulatorPilotValveFullOpenning ( 0.45)
 RegulatorMainValveInitialOpenning ( 0.44)

 SteamBlowerEffectExponent ( 0.9)
 SteamBlowerEfficiencyExponent ( 1.1)
 SteamBlowerMaxSteamUsageRate ( 500)
 SteamBlowerMaxProportionOfBlastEffect ( 0.15)

 SteamWaterScoopMinPickupSpeed( 25 ) comment( mph )
 SteamWaterScoopMaxPickupSpeed( 60 ) comment( mph )
 SteamWaterScoopResistance( 8500N )
 comment( pounds per second. 6000gallons per minute max. )
 SteamWaterScoopMaxPickupRate( 1000 )


 HeadOut ( -1.5 3.38 -6.45)

 EngineControllers (
  Regulator ( 0 1 0.0125 0
   NumNotches ( 0)
  )
  Cutoff ( -0.55 0.75 0.0125 0
   NumNotches ( 0)
  )
  Brake_Engine ( 0 1 0.0125 0
   NumNotches ( 3
    Notch ( 0 1 EngineBrakesControllerReleaseStart)
    Notch ( 0.45 1 EngineBrakesControllerHoldStart)
    Notch ( 0.5 1 EngineBrakesControllerApplyStart)
   )
  )
  Brake_Train ( 0 1 0.0125 0.55
   NumNotches ( 4
    Notch ( 0    0 TrainBrakesControllerReleaseStart)
    Notch ( 0.4  1 TrainBrakesControllerSelfLapStart)
    Notch ( 0.5  1 TrainBrakesControllerApplyStart)
    Notch ( 0.95 0 TrainBrakesControllerEmergencyStart)
   )
  )
  Brake_Hand ( 0 1 0.02 0
   NumNotches ( 0)
  )
  Firedoor ( 0 1 0.2 0.4
   NumNotches ( 0)
  )
  Sanding ( 0 1 0)
  Blower ( 0 1 0.025 0.25
   NumNotches ( 0)
  )
  HeatingTap ( 0 1 0.1 0
   NumNotches ( 0)
  )
  Shovel ( 0 1 0.15 0
   NumNotches ( 0)
  )
  DampersFront ( 0 1 0.1 0.7
   NumNotches ( 0)
  )
  DampersBack ( 0 1 0.1 0.7
   NumNotches ( 0)
  )
  Injector1Steam ( 0 1 0)
  Injector2Steam ( 0 1 0)
  Injector1Water ( 0 1 0.125 0
   NumNotches ( 0)
  )
  Injector2Water ( 0 1 0.125 0
   NumNotches ( 0)
  )

  CylinderCocks ( 0 1 1)
  Whistle ( 0 1 0)
  SmallEjectorOrCompressor ( 0 1 1)
  BellToggle ( 0 1 0)
  Headlights ( 0 1 0)
 )
  Comment(fire temp, fire mass, water mass, boiler pressure,
water level, tender_water_mass, smoke_quantity,
            tender_coal_mass, fire_condition, coal quality ) 

 EngineVariables ( 850 2000 13090 210 1.0 48500 300 1.0 0.9 0.9)

 CabView ( 231G_SNCF.cvf)
 Sound ( "231Gcab.sms" )
 Name ( "MB_231B")
 Description ( "Locomotive 231 B 037 Est Pacific \n"+
    "Compagnie d'origine Est de fourniture TP : \n"+ 
    "Année de construction : 1922\n"+
    "à Nantes par Batignoles-Chatillon\n"+
    "Compound à 4 cylindres \n"+
    "Retrait de service : juin 1966\n"+
    "Puissance : 2800CV à la jante\n"+ 
    "Masse : 103t\n"+ 
    "Vitesse maxi : 155km/h ;130 en service\n\n"+ 
    "M.Bonnard_Anim Flo_Cab Pascal Grando  2010 \n")
	)
